**Del Rey Cleaners Analysis**

* Former cleaners at 310 Culver Blvd
* Possible construction with dewatering proposed at 138 Culver Blvd
* GW flow = SE on Feb 2002
* Auto repair garage from between 1935 and 1962; then cleaners from 1962 to 2007;
* In 29-March-2014 Bowyer Environmental Consulting report:
  + Soil vapor had PCE, TCE, cis-1,2-DCE, trans-1,2-DCE & VC; also some toluene, CB & CF; V-7 was the hottest with 210,000 ug/L
  + Soil samples: PCE, TCE & cis-1,2-DCE; also 1,4-DCB in one sample; V-7 the hottest with 600,000 ug/kg
* CAO R4-2014-0143; amended 28-August-2014
  + WP due 3-December-2014
  + RPs stated they lack financial assets to fund this; RWQCB requested documentation in letter dated 24-Sept-2014; pending response